* Drogue is nose coming off, main deploy main parachute
* Schematic symbol should always be rectangle to match the data sheet.
  + Change to more readable symbol
* Change capacitor to EU symbol (two plates), and change size
  + 0603 are big enough to use with tweezers
  + 0805 big enough for 10 uF
* Change 0603 for resistors as well. 2A at the most due to the P = I^2 \*R
* Changed to double up leads for the battery to have two positives and two negatives.
* Absolute maximum input voltage for voltage divider into STM32F0 analog calculation.
* Change N-Channel MOSFET to the ground to achieve a positive GS difference
* Add connection called armed from outside world need new 7 pin.
* PullUp ~ACOK to 3.3V to check if charger is on umbilical power.
* Flip Diode Symbol in the optoisolator
* For a power supply, add a bypass cap at around 100nF for each power pin
* Add button, and add ACOK.